# <u><p style="text-align: center;"> 10-Base-T1S Demos </p></u>

# Check_10BaseT1S_Comet_AE02.vs3
![Setup](resources/Check_10Base-T1S_Comet_GP.bmp)

## <u>Showcase</u>
This setup was used with <b>RAD-Comet</b>
The received messages are filtered by MAC address. Depending on the filtered message the graphical panel shows from which "node" the data was received.
New setups for [<b>RAD-Comet2</b>](https://store.intrepidcs.com/product/rad-comet-2) and [<b>RAD-Comet3</b>](https://store.intrepidcs.com/product/rad-comet-3) also will 

## <u>Requirements</u>
* <b>RAD-Comet</b> - setup was build with RAD-Comet1
	* 10-BaseT1S - Local ID=0
* several <b>RAD-Meteor</b> including USB-C cable
	* set with individual local IDs
* <b>Cabeling</b> to connect RAD-Meteors and RAD-Comet	
	* [iX to Pigtail cable](https://store.intrepidcs.com/product/ix-pt-0.5-cable)
	* mating terminal blocks for RAD-Meteor [TBP02P1-381-02BE](https://www.digikey.com/en/products/detail/cui-devices/TBP02P1-381-02BE/10238445)
* USB-powersupply for x-<b>RAD-Meteor</b>

## <u>Used Vehicle Spy version</u>
Beta 3.9.19.3


## <u>Setup</u>
1) Connect <b>RAD-Comet</b> 10-Base-T1S port to several <b>RAD-Meteor</b>
2) Power the <b>RAD-Meteors</b> via USB
3) Connect <b>RAD-Comet</b> via USB-C to the PC

## <u>Usage</u>
1) Open the setup and check the <b>RAD-Meteors</b> MAC addesses in the AE02 network settings.\
2) Go online with Vehicle Spy. \
3) To start the individual nodes, press the yellow button and start "run".