#### [Find Repositorys](https://git.intrepidcs.de/explore/repos)

# <u>Demo RAD-Galaxy2</u>

## General showcase
Short description what will be demonstrated

* <b>VividCAN1:</b><br>
  <i>Display</i> Vehicle data (see: [Demo_Datalogger](https://git.intrepidcs.de/Andreas/Demo_Datalogger))<br>
  <i>Slider</i> to change background light <br>
  -> this information will be send to second <b><i>VividCAN2</i></b> to remotely change background light. 

  <i>CAN -> CAN2ETH GW -> ETH tapping -> ETH2CAN GW</i>
  
  <i>Push buttons</i> to send TC10 commands to SFP modules of RAD-GigaStar

* <b>Fire3/Red2:</b><br>
  Simulating Vehicle data <br>
  Embedded CAN-ETH Gateway 
 
* <b>RAD-Galaxy2:</b><br>
  Tap device - ETH1 <-> ETH2 / AE01 <-> AE02 streams

* <b>RAD-GigaStar:</b><br>
  AE simulation (saw signal) - TX on AE01, RX on AE02.<br> 
  Embedded CAN-ETH-CAN Gatewaying for CAN1/2 (see [Demo_VCAN42-Ind_CAN-ETH-GW](https://git.intrepidcs.de/Andreas/Demo_VCAN42-Ind_CAN-ETH-GW)) -> to dispaly Vehicle data on <b><i>VividCAN2</i></b><br>
 

* <b>VividCAN2:</b><br>
  Display same Vehicle data as <b><i>VividCAN1</i></b> but received ofer ethernet and ETH-CAN-GW
  Backlight can be adjusted localy or over <b><i>VividCAN1</i></b> slider

* <b>VehicleSpy connected to:</b><br>
  <i><u>Variant1:</u></i><br>
  <b>RAD-GigaStar</b> (device hosting on ETH1) to display Vehicle data (CAN->ETH)<br>
  saw signal from <b><i>RAD-GigaStar</i></b> (AE1 and AE2) and on <b>RAD-Galaxy2</b> (AE3 and AE4 - only receive side)<br>
  <i><u>Variant2:</u></i> Red2/Fire3 to show original CAn data

* <b>Wireshark</b> (with ICSCAP):<br>
  Monitoring the whole, tapped streams

## Requirements
* ["Remote" Datalogger](https://intrepidcs.com/products/data-loggers/)
  (e.g. neoVI-RED2/Fire3/Connect) <br> 
  with CoreMini [Setup](RED2_Playback_and_Log_GW.vs3) and 
  replay files [File1]('full%20trace%202022-06-10%2006-54-10-290994%20Partition%200.vsb') 
  and [File2]('full%20trace%202022-06-10%2010-26-01-291045%20Partition%200.vsb')
* Two VividCAN with CoreMini [Setup]('VividCAN%20Demo.vs3')
* [RAD-Galaxy2](https://intrepidcs.com/products/automotive-ethernet-tools/rad-galaxy-2)
* [RAD-GigaStar](https://intrepidcs.com/products/automotive-ethernet-tools/rad-gigastar-1000base-t1-active-tap-gateway-vehicle-interface) 
  with CoreMini [Setup](GigaStar_CAN-ETH-GW.vs3) <br>
  (embedded CAN-ETH-CAN Gateway and device hosting)

## Connections
* Red2/Fire3 (DWCAN01) -> VividCAN1 + Power
* Red2/Fire3 (ETH1) -> RAD-Galaxy2 (ETH1)
* RAD-Galaxy2 (AE3) -> RAD-GigaStar (AE1)
* RAD-Galaxy2 (AE4) -> RAD-GigaStar (AE2)
* RAD-Galaxy2 (ETH3) -> RAD-GigaStar (SFP-ETH1)
* RAD-GigaStar (DWCAN01) -> VividCAN2 + Power

## Setup I

### Showcase - Vehicle Spy
Individual description of setup

## Setup II 
If multiple setups are available

### Showcase - Wireshark
Individual description of setup

