# RAD-IO2 Demo
![Graphical panel](./resources/Graphical_panel.bmp)

## <u>Setup:</u>
Stack RAD-IO2 devices together
    RAD-IO2-TC
    RAD-IO2-AOUT
    RAD-IO2-AIN

## <u>Connections:</u>
- Thermocouple on "Ch7" of RAD-IO2-TC
- LED on  "Bank1 Ch3" and 
          "Bank2 Ch3" of RAD-IO2-AOUT
- Connect "Bank7 Ch1" of RAD-IO2-AOUT to 
               "AIN7" of RAD-IO2-AIN

## <u>Function:</u>
- If Temperature rises over 30°C "Ch3" jumps to 5V output
- If Temperature falls below 27°C "Ch3" returns to 0V output
- Between 27°C and 30°C the Temperature divided by 10 
  will be output on "Bank2 Ch3" as Voltage on RAD-IO2-AOUT
- In parallel the Temperature divided by 10 will be output as voltage on "Bank7 Ch1"

![Testing Expo 2023](./resources/20230612_211405.jpg)