
LIBRARY icsneolegacy

EXPORTS
	icsneoOpenPort @21
	icsneoClosePort @22
	icsneoGetMessages @23
	icsneoTxMessages @24
	icsneoFreeObject @25
	icsneoGetErrorMessages @26
	icsneoStartSockServer @29
	icsneoSendConfiguration @30
	icsneoGetSerialNumber @32
	; icsneoFindAllUSBDevices @33
	icsneoOpenPortEx @34
	icsneoStopSockServer  @35
	icsneoGetErrorInfo @36
	icsneoGetDLLVersion @37
	icsneoGetConfiguration @38
	icsneoFindAllCOMDevices @39
	icsneoGetISO15765Status @40
	icsneoSetISO15765RxParameters @41
	; icsneoSetPerformanceParameters @42
	icsneoEnableNetworkCom @ 43
	; icsneoGetPerformanceParameters @ 44
	; icsneoSetupISO15765HwSupport @ 45
	icsneoWaitForRxMessagesWithTimeOut @ 46
	; icsneoGetErrorInfoW @47
	; icsneoGetOpenPorts @ 48
	; icsneoGetPerformanceTimer @ 49
	; icsneoFindFirstFreeDevice @ 50
	icsneoJ2534Cmd @ 51

	icsneoScriptStartFBlock @ 52
	icsneoScriptStopFBlock @ 53
	icsneoScriptGetFBlockStatus @ 54
	; icsneoScriptReadTxMessage @ 55
	; icsneoScriptWriteTxMessage @ 56
	icsneoScriptStart @ 57
	icsneoScriptStop @ 58

	icsneoFindNeoDevices @ 62
	icsneoOpenNeoDevice @ 63
	; icsneoOpenNeoDeviceBySerialNumber @ 64

	icsneoForceFirmwareUpdate @ 65
	icsneoGetHWFirmwareInfo @ 66
	icsneoGetDLLFirmwareInfo @ 67

	; icsneoSetupISO15765HwSupportEx @ 68

	icsneoSetBitRate  @ 69

	; icsneoReadSDCard  @ 72
	icsneoGetTimeStampForMsg @ 73

	; icsneoWriteSDCard  @ 76

	icsneoScriptLoad @ 77
	icsneoScriptClear @ 78
	icsneoGetLastAPIError @ 79
	icsneoValidateHObject @ 80

	icsneoScriptReadAppSignal @ 81
	icsneoScriptWriteAppSignal @ 82

	; icsneoScriptReadISO15765_2_TxMessage @ 84
	; icsneoScriptWriteISO15765_2_TxMessage @ 85
	; icsneoScriptReadRxMessage @ 86
	; icsneoScriptWriteRxMessage @ 87

	icsneoScriptGetScriptStatus @ 91

	icsneoEnableNetworkRXQueue @ 94
	icsneoGetFireSettings @ 95
	icsneoSetFireSettings @ 96

	icsneoGetVCAN3Settings @ 97
	icsneoSetVCAN3Settings @ 98

	icsneoGetDeviceParameters @99
	icsneoSetDeviceParameters @100

	; icsneoSetReflashCallback @101

	; icsneoSetReflashDisplayCallbacks @102
	; icsneoClearReflashDisplayCallbacks @103

	; icsneoGetStoredFirmwareInfo @104
	; icsneoDownloadISO15765_2_TXScript @ 105
	; icsneoTransmitISO15765_2_Message @106
	; icsneoClearISO15765_2_TxScript @ 107

	icsneoGetDLLVersionEx @108

	; icsneoEnable_ISO15765_2_By_Network @ 111
	; icsneoDisable_ISO15765_2 @ 112
	; icsneoSetISO15765_2_FlowCtlID @ 113
	; icsneoClearISO15765_2_FlowCtlID @ 114
	; icsneoClearAllISO15765_2_FlowCtlIDs @ 115

	; icsneoSetContext @ 116
	; icsneoFindNeoDevicesEx @ 117
	; icsneoOpenNeoDeviceEx @ 118

	icsneoFindRemoteNeoDevices @ 120
	icsneoOpenRemoteNeoDevice  @ 121
	icsneoISO15765_EnableNetworks @122
	icsneoISO15765_DisableNetworks @123
	icsneoISO15765_TransmitMessage @124

	icsneoGetCANControllerClockFrequency @129
	icsneoSetCANParameters @130
	icsneoSetCANParametersPhilipsSJA1000 @131

	; icsneoSendTextApi @132
	; icsneoGetTextApi @133
	; icsneoScriptReadISO15765_2_RxMessage @ 134
	; icsneoScriptWriteISO15765_2_RxMessage @ 135

	; icsneoScriptLoadReadBin @ 136
	; icsneoEnableCoreMiniUsbFilter @ 137
	; icsneoConfigureNetworkMsgQueue @ 138
	icsneoEnableBusVoltageMonitor @ 139
	icsneoGetBusVoltage @ 140
	icsneoEnableBitSmash @141
	icsneoDisableBitSmash @142
	icsneoReceiveHWTimeResponse @143
	icsneoSendHWTimeRequest @144
	icsneoSetUSBLatency     @145
	; icsneoLoadDefaultSettings @146
	; icsneoGetAllChipVersions @149
	icsneoSetBitRateEx  @ 150
	; icsneoScriptGetScriptStatusEx  @ 151
	icsneoOpenNeoDeviceByChannels @ 152
	; icsneoGetChannelLockStatus @ 153
	; icsneoRequestEnterSleepMode @ 154
	icsneoEnableNetworkComEx @ 155
	; icsneoLockChannels @ 156
	; icsneoUnlockChannels @ 157

	; icsneoGetFireVnetSettings @ 160
	; icsneoSetFireVnetSettings @ 161

	icsneoGetFire2Settings @ 162
	icsneoSetFire2Settings @ 163
	icsneoSetFDBitRate @ 164

	icsneoTxMessagesEx @165

	icsneoGetVCANRFSettings @ 167
	icsneoSetVCANRFSettings @ 168

	icsneoFirmwareUpdateRequired @ 169

	icsneoGetRADGalaxySettings @170
	icsneoSetRADGalaxySettings @171

	icsneoGetNetidforSlaveVNETs @172
	icsneoGetVnetSimpleNetid @173
	icsneoISO15765_ReceiveMessage @174
	icsneoGetDLLFirmwareInfoEx @175
	; icsneoBase36enc @176
	icsneoGetRADStar2Settings @177
	icsneoSetRADStar2Settings @178

	; icsneoGetBackupPowerEnabled @179
	; icsneoSetBackupPowerEnabled @180
	; icsneoGetBackupPowerReady @181
	icsneoSerialNumberFromString @182
	icsneoSerialNumberToString @183
	icsneoISO15765_TransmitMessageEx @184

	; icsneoGetActiveVNETChannel @ 189
	; icsneoSetActiveVNETChannel @ 190

	icsneoGetDeviceSettings @191
	icsneoSetDeviceSettings @192
	icsneoGetDeviceSettingsType @193

	icsneoGetVCAN412Settings @ 194
	icsneoSetVCAN412Settings @ 195

	; icsneoGetVividCANSettings @ 196
	; icsneoSetVividCANSettings @ 197
	; icsneoFindNeoDevicesNewStyle @ 198

	; icsneoGetDeviceStatus @ 202

	icsneoFindDevices @ 203
	icsneoOpenDevice @ 204

	icsneoEnableDOIPLine @ 205
	icsneoGetMiniportAdapterInfo @ 206

	icsneoGetVCAN4Settings @ 207
	icsneoSetVCAN4Settings @ 208

	; icsneoReadWritePHYSettings @ 214

	; icsneoRequestDiskDetails @ 217
	; icsneoRequestDiskFormat @ 218
	; icsneoRequestDiskFormatProgress @ 219
	; icsneoRequestDiskFormatCancel @ 220

	; icsneoGetRADGigastarSettings @ 221
	; icsneoSetRADGigastarSettings @ 222
	; icsneoGetRADA2BSettings @ 223
	; icsneoSetRADA2BSettings @ 224

	; icsneoScriptClearRxMessage @225